Requirement :
2 Computers with local network and internet link
- 1st computer Pegasos1 or 2/Amiga with PCI Bus
- 2nd computer PC/Pegasos1 or 2/Amiga ...
- 1 Switch or 1 Hub for local network
- openpci.library v2.0 or more
- openpci_8139.device v1.03b
- a ftp client on 1st computer
- a ftp server on 2nd computer

What you need to do:
1) Quote in a file all hardware used :
Example
1st computer: 
- Pegasos 1 @ 700Mhz with 256MB SDRAM
- MorphOS v1.4
- Network card : RTL8139D
- AmiTradeCenter for ftp client
2nd computer: 
- PC AthlonXP 1800+ with 512MB SDRAM
- WindowsXp
- Network card : 3COM - 3C905C-TX
- Serv-U v5.0 for ftp server

Hardware Hub or Switch used in local network:
- Edimax Hub Dual Speed 10/100Mb, 8 ports

2) Install openpci.library v2.0 or more & openpci_8139.device in the 1st computer
Device driver Install:
----------------------
For MorphOS users:
Use the native PPC MOS version openpci_8139.device.elf
- copy openpci_8139.device.elf mossys:devs/networks/openpci_8139.device
Becareful it must be copied as openpci_8139.device because if it's called openpci_8139.device.elf it will don't work
For AmigaOS users:
Use the 68k version openpci_8139.device
- copy openpci_8139.device devs:networks/openpci_8139.device
Config File Install :
---------------------
- make a dir OpenPCI in Envarc: if it doesn't exist
- copy the file openpci_8139_0.config in Envarc:OpenPCI/

--------------------------------- TEST 1 ------------------------------------------------
3) Configure the openpci 8139 driver 
- In your TCP/IP Stack verify the openpci 8139 driver is Offline or set it to Offline mode
- With a text editor edit file Env:OpenPCI/openpci_8139_0.config
Set the value to 0
It's Speed Auto Negociation
- In your TCP/IP Stack set the openpci 8139 drive to Online mode

4) Transfert a huge file 100MBytes minimum
 from 2nd computer -> 1st computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared

5) Transfert a huge file 100MBytes minimum
 from 1nd computer -> 2nd computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared

--------------------------------- TEST 2 ------------------------------------------------
6) Configure the openpci 8139 driver 
- In your TCP/IP Stack verify the openpci 8139 driver is Offline or set it to Offline mode
- With a text editor edit file Env:OpenPCI/openpci_8139_0.config
Set the value to 1
It's 10Mb Half-Duplex
- In your TCP/IP Stack set the openpci 8139 drive to Online mode

7) Transfert a huge file 100MBytes minimum
 from 2nd computer -> 1st computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared

8) Transfert a huge file 100MBytes minimum
 from 1nd computer -> 2nd computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared

--------------------------------- TEST 3 ------------------------------------------------
9) Configure the openpci 8139 driver 
- In your TCP/IP Stack verify the openpci 8139 driver is Offline or set it to Offline mode
- With a text editor edit file Env:OpenPCI/openpci_8139_0.config
Set the value to 2
It's 10Mb Full-Duplex
- In your TCP/IP Stack set the openpci 8139 drive to Online mode

10) Transfert a huge file 100MBytes minimum
 from 2nd computer -> 1st computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared

11) Transfert a huge file 100MBytes minimum
 from 1nd computer -> 2nd computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared

--------------------------------- TEST 4 ------------------------------------------------
12) Configure the openpci 8139 driver 
- In your TCP/IP Stack verify the openpci 8139 driver is Offline or set it to Offline mode
- With a text editor edit file Env:OpenPCI/openpci_8139_0.config
Set the value to 3
It's 100Mb Half-Duplex
- In your TCP/IP Stack set the openpci 8139 drive to Online mode

13) Transfert a huge file 100MBytes minimum
 from 2nd computer -> 1st computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared

14) Transfert a huge file 100MBytes minimum
 from 1nd computer -> 2nd computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared

--------------------------------- TEST 5 (the last ;-) ----------------------------------
12) Configure the openpci 8139 driver 
- In your TCP/IP Stack verify the openpci 8139 driver is Offline or set it to Offline mode
- With a text editor edit file Env:OpenPCI/openpci_8139_0.config
Set the value to 4
It's 100Mb Full-Duplex
- In your TCP/IP Stack set the openpci 8139 drive to Online mode

13) Transfert a huge file 100MBytes minimum
 from 2nd computer -> 1st computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared

14) Transfert a huge file 100MBytes minimum
 from 1nd computer -> 2nd computer 
- Quote the exact file size transfered, time in second and speed in Kbytes/sec
- If any problem occurs write what has appeared
