News/Fixes in V2.1
- Grex & Pegasos1/2 : Fixed a bug in pci_read_config_long() who return bad result for registernum >16 (Thanks to Guido Mersmann)
- Add Mediator1200SX support (Thanks to Thomas Siegel)
- Prometheus : Fixed IO or Mem Address detection bit in base_size (Bit0 set to 1=IO Address, Bit0 set to 0=Mem Address) (Titan)
- Prometheus : Fixed Read/WriteConfXXX, pci_physic_to_logic_addr, pci_set_master & 
    pci_obtain_card/pci_release_card requires prometheus.library v3 (Titan)
- Pegasos1/2 & Grex : Fixed Address base value for ROM, pci_obtain_card/pci_release_card bug/crash (Titan)
- Mediator : Fixed pci_obtain_card/pci_release_card (Titan)
- Amithlon : Fixed pci_obtain_card/pci_release_card (Titan)

News in V2.0

- New functions : pci_physic_to_logic_addr()/pci_obtain_card()/pci_release_card()
- This version is fully compatible with old drivers developped for openpci v1.x but i advise you
to support new pci card lock mechanism (pci_obtain_card()/pci_release_card()) to avoid problems 
with drivers who use the same pci card.
- Fixed read & write_config for Prometheus
- Use lock mechanism of Prometheus, Amithlon, Grex
Warning this library support Mediator and i haven't tested it on 
Mediator, Prometheus, Grex, Amithlon but it could work.
Please test and send me feedback for Mediator, Prometheus, Grex, Amithlon, Pegasos1 & Pegasos2.

Informations:

The openpci.library currently support fully Mediator, Pegasos, GrexA1200, GrexA4000, Amithlon
Prometheus wrapper is finished but need more testing.

openpci.library.elf :
- This is for MorphOS and Pegasos, it's a PPC MorphOS native version.
- This native PPC MorphOS native version support Pegasos, GrexA1200, GrexA4000, Prometheus PCI Bus

For Pegasos use openpci.library.elf ONLY and remove openpci.library if it exist,
because openpci.library doesn't support Pegasos.

openpci.library:
- This is a 68k version for AmigaOS 3.x and Amithlon
- This version support Mediator, GrexA1200, GrexA4000, Prometheus, PC PCI Bus under Amithlon.

Requirements:

To use openpci.library driver with GrexA1200-A4000 or Pegasos board you need:
cybpci.library v2.x or more
68040 or 68060.library by Ralph Schmidt v44 or more 
You can download all this files to: 
http://www.vgr.com/grex/

To use openpci.library driver with Prometheus board you need:
prometheus.library v3.x or more

To use openpci.library driver with Amithlon board you need:
powerpci.library v2.xx or more

